** fcgkj jkT; 'kS{kf.kd vk/kkjHkwr lajpuk fodkl fuxe fyfeVsM**

**BIHAR STATE EDUCATIONAL INFRASTRUCTURE DEVELOPMENT CORPORATION LTD.**

( A Govt. of Bihar Undertaking )

ISO 9001:14001;OHSAS 18001

Shiksha Bhawan, Bihar Rashtrabhasa, Parishad Campus, Acharya Shivpujan Sahay Path, Saidpur, Patna-800004

Tel. No : 0612 - 2660850 \*Fax No : 0612 - 2660256

E-mail: bseidc@gmail.com \* Website : http:/www.bseidc.in \* CIN: U80301BR2010SGC015859

**nj vkea=.k gsrq vYidkyhu dksVs’ku vkea=.k lwpuk la[;k&21 o"kZ&2020&21**

fcgkj jkT; 'kS{kf.kd vk/kkjHkwr lajpuk fodkl fuxe fyŒ iVuk ds fucaf/kr laosndksa@[;kfr izkIr QeksZa@daifu;ksa ls fnukad%& 22-09-2020 ds vijkgu 03%00 cts rd jkT; ds fofHkUu ftykUrxZr fofHkUu fuekZ.k dk;ksZ esa iz;ksx gsrq Playing Equipment ls lacaf/kr dk;ksZ gsrq xSj vuqlwfpr enksa dh vkiwfrZ ,oa vf/k"Bkiu ds fy, fuEukafdr enksa gsrq eqgjcan dksVs’ku v/kh{k.k vfHk;ark] fcgkj jkT; 'kS{kf.kd vk/kkjHkwr lajpuk fodkl fuxe fyŒ] iVuk ds dk;kZy; esa izkIr fd;k tk,xk ,oa mlh fnu vijkgu 03%30 cts dksVs’kunkrkvksa ;k muds vf/kd`r izfrfuf/k;ksa ds le{k [kksyk tk,xkA

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Sl. No.** | **Description of items** | **Qty** | **Unit** | **Rate  (In Digits)** | **Rate ( In Words )** |
| 1 | Supplying of Yoga Mat/Exercise Mat having size of 180cm (L) X 90cm (W) X 12mm (T), Material- Ethylene Vinyl Acetate of approved colour and texture all complete job as per direction of EI. | 1.00 | Each |  |  |
| 2 | Supply and installation of multi colour EPDM Rubber Flooring having thickness of 25 mm for polymeric sports surface to existing surface as per design & drawing, as per technical specifications including carriage and necessary required equipment all complete job as per direction of E/I | 1.00 | Sqm |  |  |
| 3 | Supplying & Installation of rosewood Carrom board made up of Lacquered Plywood Playing Surface (Side of Square) 73.5 cm to 74 cm, thickness of Playing Surface (Min) 8 mm as per design & drawing, as per technical specifications including carriage and necessary required equipment all complete job as per direction of E/I | 1.00 | Each |  |  |
| 4 | Supply and installation of AB Climber , Type of slide ladder : Full Arch shape Slide ladder made up of virgin grade polyethylene plastic as per design & drawing, as per technical specifications including carriage and necessary required equipment all complete job as per direction of E/I | 1.00 | Each |  |  |
| 5 | Supply and installation of one set of swing of 2 seater 9 ft high (one set of swing of 2 seater 9 ft high)Swing seat made up of Virgin grade polyethylene plastic as per design & drawing, as per technical specifications including carriage and necessary required equipment all complete job as per direction of E/I | 1.00 | Each |  |  |
| 6 | Supply and installation ofOutdooor gym horse rider, Type : Leg Press Single Maximum User Weight ( Kg ) : 100 kilogram as per design & drawing, as per technical specifications including carriage and necessary required equipment all complete job as per direction of E/I | 1.00 | Each |  |  |
| 7 | Supply and installation of Indoor Fun See Saw having size of Size of see saw(L x H X base width) (in mm) 1265 x 400 x 400,Size of base of see saw(L x H) (in mm) 400 x 145,Uppertop and bottom width of base of see saw(W x W) (in mm) 60 x 80,Thickness of item(in mm) 2.5,Height of Button mushroom mechanism fitting(in mm) 125, Top and bottom diameter of Button mushroom mechanism fitting(D x D)(in mm) 150 x 40,Size of upper side of Button mushroom mechanism fitting(L x W x D)(in mm) 100 x 35 x 65, Size of middle part of see saw(L x H x W x T)(in mm) 510 x 225 x 55 x 4,Diameter of see saw seat hole(in mm) 7,Space between 7mm and 40mm diameter(in mm) 35,Base Locking(W x H)(in mm) 95 x 70,Size of See saw seat (L x W)(in mm) 540 x 90,Handle(L x Dia x T)(in mm) 260 x 25 x 4 Total seating base(in mm) 220,Gap between handle and front side(in mm) 140 Size of seating base(bottom)(Dia x Dep)(in mm) 90 x 50,Diameter of rubber balloon after blowing(in mm) 180,Height of MS bolt(in mm) 20 Diameter of MS bolt (2 piece) (in mm) 7 Diameter of MS bolt (4 nos)(in mm) 50 Inner diameter (in mm) 10,Thickness (2 piece)(in mm) 2,Height of screw(4 nos)(in mm) 10 Diameter of align key(in mm) 4 complete as per design & drawing, as per technical specifications including carriage and necessary required equipment all complete job as per direction of E/I | 1.00 | Each |  |  |

**fo'ks"k 'krsZ&**

* ;g dksVs’ku flQZ nj fu/kkZj.k gsrq vkeaf=r fd;k x;k gSA
* dksVs’kunkrkvksa dks viuk nj ¼lHkh djksa] GST ,oa <qykbZ O;; ds lkFk½ vad ,oa v{kjksa esa m)`r djuk gksxkA
* fo’ks"k lwpuk ds fy, lwpukiV~V ;k osclkbV [www.prdbihar.gov.in](http://www.prdbihar.gov.in) ,oa [www.bseidc.in](http://www.bseidc.in) ns[ksa vFkok v/kksgLrk{kjh ds dk;kZy; esa dk;kZof/k esa laidZ fd;k tk ldrk gSA

**v/kh{k.k vfHk;ark**

**BSEIDC, iVukA**